(export (version D)
  (design
    (source /home/jens/work/HendiControl/Control/PCB/HendiControl/HendiControl.sch)
    (date "Mi 06 Mär 2019 17:56:50 CET")
    (tool "Eeschema 5.0.0+dfsg1-2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source HendiControl.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U5)
      (value ATmega328P-AU)
      (footprint Package_QFP:TQFP-32_7x7mm_P0.8mm)
      (datasheet https://www.microchip.com/wwwproducts/en/ATmega328)
      (libsource (lib MCU_Microchip_ATmega) (part ATmega328P-AU) (description "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-32"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61F184))
    (comp (ref L1)
      (value "Ferrite Bead")
      (footprint Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with Ferrite Core"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6222E4))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C622402))
    (comp (ref Y2)
      (value 18.432MHz)
      (footprint Crystal:Crystal_HC49-4H_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62E497))
    (comp (ref C15)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6335F0))
    (comp (ref C10)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63A718))
    (comp (ref R11)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6563D3))
    (comp (ref C16)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C659808))
    (comp (ref D2)
      (value RX-LED)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C683697))
    (comp (ref D1)
      (value TX-LED)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6838FA))
    (comp (ref R8)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C692B19))
    (comp (ref R9)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C692BB5))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63FB29))
    (comp (ref R12)
      (value 100R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C66E319))
    (comp (ref J5)
      (value Debugwire)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x03_Odd_Even) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C679FFD))
    (comp (ref C13)
      (value 18p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6DA82A))
    (comp (ref C14)
      (value 18p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6DA8CA))
    (comp (ref R17)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6CBE3B))
    (comp (ref C5)
      (value 10u/16V)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6F4F66))
    (comp (ref C17)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C731273))
    (comp (ref C19)
      (value 10u/16V)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C73127F))
    (comp (ref C8)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7AEE30))
    (comp (ref U3)
      (value ISO7221)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7321c&fileType=pdf)
      (libsource (lib Isolator) (part ISO7321C) (description "Low Power Dual-Channel 1/1 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C888A4D))
    (comp (ref C9)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C994409))
    (comp (ref C11)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9944E2))
    (comp (ref SW1)
      (value Reset-Switch)
      (footprint Button_Switch_SMD:SW_SPST_PTS645)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA205BF))
    (comp (ref U4)
      (value MCP47x6)
      (footprint Package_TO_SOT_SMD:SOT-23-6_Handsoldering)
      (libsource (lib MyLib) (part MCP47x6) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA6A8A1))
    (comp (ref R15)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB2D42F))
    (comp (ref R14)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB2D4D3))
    (comp (ref J2)
      (value Isolation-Bypass)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x02_Odd_Even) (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDD2E9F))
    (comp (ref R13)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEABD73))
    (comp (ref C18)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEF111C))
    (comp (ref MH2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF45D6A))
    (comp (ref MH1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF4600C))
    (comp (ref MH3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF460B2))
    (comp (ref MH4)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF46142))
    (comp (ref C12)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEA028D))
    (comp (ref C3)
      (value 10n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA465E5))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB64B9B))
    (comp (ref U2)
      (value ISO7220)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7320c&fileType=pdf)
      (libsource (lib Isolator) (part ISO7320C) (description "Low Power Dual-Channel 2/0 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD0A18F))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF719A5))
    (comp (ref J6)
      (value USB-Conn)
      (footprint Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical)
      (datasheet https://www.reichelt.de/stiftleiste-2-54-mm-1x05-gerade-rnd-205-00674-p210918.html?&trstct=pol_13)
      (libsource (lib Connector_Generic) (part Conn_01x05) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D11F58F))
    (comp (ref J1)
      (value Hendi-Poti)
      (footprint Connector_JST:JST_XH_S04B-XH-A-1_1x04_P2.50mm_Horizontal)
      (datasheet https://www.reichelt.de/jst-stiftleiste-90-1x4-polig-xh-jst-xh4p-st90-p185081.html?&trstct=pol_13)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1C3F81))
    (comp (ref J3)
      (value "Hendi Mainboard")
      (footprint Connector_JST:JST_XH_S04B-XH-A-1_1x04_P2.50mm_Horizontal)
      (datasheet https://www.reichelt.de/jst-stiftleiste-90-1x4-polig-xh-jst-xh4p-st90-p185081.html?&trstct=pol_13)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1CFC96))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6B6044))
    (comp (ref U1)
      (value FT232RL)
      (footprint Package_SO:SSOP-28_5.3x10.2mm_P0.65mm)
      (datasheet http://www.ftdichip.com/Products/ICs/FT232RL.htm)
      (libsource (lib MyLib) (part FT232RL) (description "USB to Serial Interface, SSOP-28"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D2D2714))
    (comp (ref D3)
      (value HB)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D39E334))
    (comp (ref R4)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D39F0EB))
    (comp (ref D4)
      (value PWRSWITCHLED)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D45E1DF))
    (comp (ref R5)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D45E2D7))
    (comp (ref Q2)
      (value BC847B)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657)
      (libsource (lib Transistor_BJT) (part BC847) (description "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C833961))
    (comp (ref Q3)
      (value BC847B)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657)
      (libsource (lib Transistor_BJT) (part BC847) (description "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B0AF))
    (comp (ref R6)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C84B451))
    (comp (ref R20)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C900BB2))
    (comp (ref JP2)
      (value BootSel)
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_3_Open) (description "Solder Jumper, 3-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C980058))
    (comp (ref C4)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC2A06F))
    (comp (ref C7)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC2A075))
    (comp (ref R3)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCD393F))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCD3A4B))
    (comp (ref JP3)
      (value AVCC)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD62A7D))
    (comp (ref JP4)
      (value DAREF)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD80A8B))
    (comp (ref JP5)
      (value AREF)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD80CAA))
    (comp (ref JP1)
      (value MCURST)
      (footprint Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_3_Open) (description "Solder Jumper, 3-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C97FCEB))
    (comp (ref Q1)
      (value IRF7416)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.infineon.com/dgdl/irf7416pbf.pdf?fileId=5546d462533600a4015355fac5661bc6)
      (libsource (lib Transistor_FET) (part IRF7404) (description "-6.7A Id, -20V Vds, P-Channel HEXFET Power MOSFET, SO-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C850557))
    (comp (ref L2)
      (value Ferrite)
      (footprint Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Core_Ferrite) (description "Inductor with Ferrite Core"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C81A2EE))
    (comp (ref C20)
      (value 10n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C93B020))
    (comp (ref D9)
      (value BSEL)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAEEDE2))
    (comp (ref D10)
      (value ERR)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAEF1B0))
    (comp (ref D7)
      (value LED2)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAEF25E))
    (comp (ref D8)
      (value LED3)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAEF308))
    (comp (ref R22)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB7CB9D))
    (comp (ref R23)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB7CCB7))
    (comp (ref R19)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB7CD69))
    (comp (ref R21)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB7CE15))
    (comp (ref D5)
      (value LED0)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD948A8))
    (comp (ref D6)
      (value LED1)
      (footprint LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD948AE))
    (comp (ref R16)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD948B4))
    (comp (ref R18)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD948BA))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEB3636))
    (comp (ref C21)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF09144))
    (comp (ref C22)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CFE9A0C))
    (comp (ref C23)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D00E3A4)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x05)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x02_Odd_Even)
      (description "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x02_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x03_Odd_Even)
      (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x03_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "LED generic")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part L_Core_Ferrite)
      (description "Inductor with Ferrite Core")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L_Core_Ferrite))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Isolator) (part ISO7320C)
      (aliases
        (alias ISO7320FC))
      (description "Low Power Dual-Channel 2/0 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8")
      (docs http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7320c&fileType=pdf)
      (footprints
        (fp SO*))
      (fields
        (field (name Reference) U)
        (field (name Value) ISO7320C)
        (field (name Footprint) Package_SO:SOIC-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name VCC1) (type power_in))
        (pin (num 2) (name INA) (type input))
        (pin (num 3) (name INB) (type input))
        (pin (num 4) (name GND1) (type power_in))
        (pin (num 5) (name GND2) (type power_in))
        (pin (num 6) (name OUTB) (type output))
        (pin (num 7) (name OUTA) (type output))
        (pin (num 8) (name VCC2) (type power_in))))
    (libpart (lib Isolator) (part ISO7321C)
      (aliases
        (alias ISO7321FC))
      (description "Low Power Dual-Channel 1/1 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8")
      (docs http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7321c&fileType=pdf)
      (footprints
        (fp SO*))
      (fields
        (field (name Reference) U)
        (field (name Value) ISO7321C)
        (field (name Footprint) Package_SO:SOIC-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name VCC1) (type power_in))
        (pin (num 2) (name OUTA) (type output))
        (pin (num 3) (name INB) (type input))
        (pin (num 4) (name GND1) (type power_in))
        (pin (num 5) (name GND2) (type power_in))
        (pin (num 6) (name OUTB) (type output))
        (pin (num 7) (name INA) (type input))
        (pin (num 8) (name VCC2) (type power_in))))
    (libpart (lib Jumper) (part SolderJumper_2_Open)
      (description "Solder Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_3_Open)
      (description "Solder Jumper, 3-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_3_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib MCU_Microchip_ATmega) (part ATmega48A-AU)
      (aliases
        (alias ATmega48PA-AU)
        (alias ATmega88A-AU)
        (alias ATmega88PA-AU)
        (alias ATmega168A-AU)
        (alias ATmega168PA-AU)
        (alias ATmega328-AU)
        (alias ATmega328P-AU))
      (description "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf)
      (footprints
        (fp TQFP*7x7mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATmega48A-AU)
        (field (name Footprint) Package_QFP:TQFP-32_7x7mm_P0.8mm))
      (pins
        (pin (num 1) (name PD3) (type BiDi))
        (pin (num 2) (name PD4) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name VCC) (type passive))
        (pin (num 7) (name XTAL1/PB6) (type BiDi))
        (pin (num 8) (name XTAL2/PB7) (type BiDi))
        (pin (num 9) (name PD5) (type BiDi))
        (pin (num 10) (name PD6) (type BiDi))
        (pin (num 11) (name PD7) (type BiDi))
        (pin (num 12) (name PB0) (type BiDi))
        (pin (num 13) (name PB1) (type BiDi))
        (pin (num 14) (name PB2) (type BiDi))
        (pin (num 15) (name PB3) (type BiDi))
        (pin (num 16) (name PB4) (type BiDi))
        (pin (num 17) (name PB5) (type BiDi))
        (pin (num 18) (name AVCC) (type power_in))
        (pin (num 19) (name ADC6) (type input))
        (pin (num 20) (name AREF) (type input))
        (pin (num 21) (name GND) (type passive))
        (pin (num 22) (name ADC7) (type input))
        (pin (num 23) (name PC0) (type BiDi))
        (pin (num 24) (name PC1) (type BiDi))
        (pin (num 25) (name PC2) (type BiDi))
        (pin (num 26) (name PC3) (type BiDi))
        (pin (num 27) (name PC4) (type BiDi))
        (pin (num 28) (name PC5) (type BiDi))
        (pin (num 29) (name ~RESET~/PC6) (type BiDi))
        (pin (num 30) (name PD0) (type BiDi))
        (pin (num 31) (name PD1) (type BiDi))
        (pin (num 32) (name PD2) (type BiDi))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) MH)
        (field (name Value) MountingHole)))
    (libpart (lib MyLib) (part FT232RL)
      (description "USB to Serial Interface, SSOP-28")
      (docs http://www.ftdichip.com/Products/ICs/FT232RL.htm)
      (footprints
        (fp SSOP*5.3x10.2mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) FT232RL)
        (field (name Footprint) Package_SO:SSOP-28_5.3x10.2mm_P0.65mm))
      (pins
        (pin (num 1) (name TXD) (type output))
        (pin (num 2) (name DTR) (type output))
        (pin (num 3) (name RTS) (type output))
        (pin (num 4) (name VCCIO) (type input))
        (pin (num 5) (name RXD) (type input))
        (pin (num 6) (name RI) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 9) (name DCR) (type input))
        (pin (num 10) (name DCD) (type input))
        (pin (num 11) (name CTS) (type input))
        (pin (num 12) (name CBUS4) (type BiDi))
        (pin (num 13) (name CBUS2) (type BiDi))
        (pin (num 14) (name CBUS3) (type BiDi))
        (pin (num 15) (name USBD+) (type BiDi))
        (pin (num 16) (name USBD-) (type BiDi))
        (pin (num 17) (name 3V3OUT) (type input))
        (pin (num 18) (name GND) (type power_in))
        (pin (num 19) (name ~RESET~) (type input))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name CBUS1) (type output))
        (pin (num 23) (name CBUS0) (type BiDi))
        (pin (num 25) (name AGND) (type power_in))
        (pin (num 26) (name TEST) (type power_in))
        (pin (num 27) (name OSCI) (type input))
        (pin (num 28) (name OSCO) (type output))))
    (libpart (lib MyLib) (part MCP47x6)
      (fields
        (field (name Reference) U)
        (field (name Value) MCP47x6))
      (pins
        (pin (num 1) (name VOUT) (type output))
        (pin (num 2) (name VSS) (type power_in))
        (pin (num 3) (name VDD) (type power_in))
        (pin (num 4) (name SDA) (type input))
        (pin (num 5) (name SCL) (type input))
        (pin (num 6) (name VREF) (type power_in))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Transistor_BJT) (part BC817)
      (aliases
        (alias BC818)
        (alias BC847)
        (alias BC848)
        (alias BC849)
        (alias BC850)
        (alias MMBT3904)
        (alias MMBT5550L)
        (alias MMBT5551L))
      (description "0.8A Ic, 45V Vce, NPN Transistor, SOT-23")
      (docs http://www.fairchildsemi.com/ds/BC/BC817.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC817)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transistor_FET) (part IRF7404)
      (description "-6.7A Id, -20V Vds, P-Channel HEXFET Power MOSFET, SO-8")
      (docs http://www.infineon.com/dgdl/irf7404.pdf?fileId=5546d462533600a4015355fa2b5b1b9e)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) Q)
        (field (name Value) IRF7404)
        (field (name Footprint) Package_SO:SOIC-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name S) (type passive))
        (pin (num 4) (name G) (type passive))
        (pin (num 5) (name D) (type passive))
        (pin (num 6) (name D) (type passive))
        (pin (num 7) (name D) (type passive))
        (pin (num 8) (name D) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Isolator)
      (uri /usr/share/kicad/library/Isolator.lib))
    (library (logical Jumper)
      (uri /usr/share/kicad/library/Jumper.lib))
    (library (logical MCU_Microchip_ATmega)
      (uri /usr/share/kicad/library/MCU_Microchip_ATmega.lib))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical MyLib)
      (uri /home/jens/work/HendiControl/Control/PCB/HendiControl/MyLib.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Transistor_BJT)
      (uri /usr/share/kicad/library/Transistor_BJT.lib))
    (library (logical Transistor_FET)
      (uri /usr/share/kicad/library/Transistor_FET.lib)))
  (nets
    (net (code 1) (name +5VD)
      (node (ref R19) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref R23) (pin 1))
      (node (ref J5) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U5) (pin 4))
      (node (ref U5) (pin 6))
      (node (ref R21) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref R22) (pin 1))
      (node (ref JP5) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref R14) (pin 1))
      (node (ref JP3) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref L2) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref C21) (pin 1)))
    (net (code 2) (name /BOOTSEL)
      (node (ref JP2) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref R6) (pin 1)))
    (net (code 3) (name /MCURST)
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref JP1) (pin 3)))
    (net (code 4) (name /#HBLED)
      (node (ref D3) (pin 1))
      (node (ref U5) (pin 14)))
    (net (code 5) (name GNDD)
      (node (ref U5) (pin 5))
      (node (ref C17) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C20) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C23) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref C22) (pin 2))
      (node (ref JP1) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref JP2) (pin 3))
      (node (ref C11) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref U5) (pin 21))
      (node (ref U5) (pin 3))
      (node (ref J1) (pin 4))
      (node (ref J3) (pin 1))
      (node (ref C16) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref SW1) (pin 1))
      (node (ref J5) (pin 6)))
    (net (code 6) (name "Net-(D4-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 7) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 8) (name /DTR)
      (node (ref U1) (pin 2))
      (node (ref U2) (pin 3)))
    (net (code 9) (name /RTS)
      (node (ref U2) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 10) (name "Net-(Q3-Pad1)")
      (node (ref R6) (pin 2))
      (node (ref Q3) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 11) (name /#BOOTSEL)
      (node (ref U5) (pin 13))
      (node (ref R20) (pin 1))
      (node (ref Q3) (pin 3)))
    (net (code 12) (name /#RST)
      (node (ref SW1) (pin 2))
      (node (ref J5) (pin 5))
      (node (ref U5) (pin 29))
      (node (ref Q2) (pin 3))
      (node (ref R17) (pin 1)))
    (net (code 13) (name GNDA)
      (node (ref C5) (pin 2))
      (node (ref U1) (pin 26))
      (node (ref J2) (pin 3))
      (node (ref U1) (pin 25))
      (node (ref U1) (pin 7))
      (node (ref C6) (pin 1))
      (node (ref U1) (pin 18))
      (node (ref U1) (pin 21))
      (node (ref C8) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref J6) (pin 4))
      (node (ref J6) (pin 5))
      (node (ref U2) (pin 4))
      (node (ref C9) (pin 1))
      (node (ref U3) (pin 4))
      (node (ref C2) (pin 1)))
    (net (code 14) (name +5VA)
      (node (ref U2) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref U3) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 20)))
    (net (code 15) (name "Net-(Q2-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref Q2) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 16) (name /VBUS)
      (node (ref L1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref J6) (pin 1)))
    (net (code 17) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 18) (name "Net-(U1-Pad27)")
      (node (ref U1) (pin 27)))
    (net (code 19) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 20) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 21) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 22) (name "Net-(C6-Pad2)")
      (node (ref U1) (pin 17))
      (node (ref C6) (pin 2)))
    (net (code 23) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 24) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 25) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 26) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 27) (name /#ELED)
      (node (ref D10) (pin 1))
      (node (ref U5) (pin 11)))
    (net (code 28) (name /#MLED)
      (node (ref D9) (pin 1))
      (node (ref U5) (pin 10)))
    (net (code 29) (name /#LED0)
      (node (ref D5) (pin 1))
      (node (ref U5) (pin 32)))
    (net (code 30) (name /#LED1)
      (node (ref D6) (pin 1))
      (node (ref U5) (pin 1)))
    (net (code 31) (name /#LED2)
      (node (ref D7) (pin 1))
      (node (ref U5) (pin 2)))
    (net (code 32) (name /#LED3)
      (node (ref D8) (pin 1))
      (node (ref U5) (pin 9)))
    (net (code 33) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref R18) (pin 2)))
    (net (code 34) (name "Net-(D5-Pad2)")
      (node (ref D5) (pin 2))
      (node (ref R16) (pin 2)))
    (net (code 35) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref U4) (pin 1)))
    (net (code 36) (name /#RXLED)
      (node (ref D2) (pin 1))
      (node (ref U1) (pin 22)))
    (net (code 37) (name /#TXLED)
      (node (ref U1) (pin 23))
      (node (ref D1) (pin 1)))
    (net (code 38) (name /USB-)
      (node (ref J6) (pin 2))
      (node (ref U1) (pin 16)))
    (net (code 39) (name /USB+)
      (node (ref J6) (pin 3))
      (node (ref U1) (pin 15)))
    (net (code 40) (name /EM_BS)
      (node (ref Q3) (pin 2))
      (node (ref JP1) (pin 2)))
    (net (code 41) (name /EM_RST)
      (node (ref JP2) (pin 2))
      (node (ref Q2) (pin 2)))
    (net (code 42) (name "Net-(C20-Pad2)")
      (node (ref L2) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref C20) (pin 2)))
    (net (code 45) (name "Net-(D10-Pad2)")
      (node (ref D10) (pin 2))
      (node (ref R23) (pin 2)))
    (net (code 46) (name "Net-(D9-Pad2)")
      (node (ref R22) (pin 2))
      (node (ref D9) (pin 2)))
    (net (code 47) (name "Net-(D7-Pad2)")
      (node (ref R19) (pin 2))
      (node (ref D7) (pin 2)))
    (net (code 48) (name "Net-(D8-Pad2)")
      (node (ref R21) (pin 2))
      (node (ref D8) (pin 2)))
    (net (code 49) (name /SCK)
      (node (ref U5) (pin 17))
      (node (ref J5) (pin 3)))
    (net (code 50) (name /MISO)
      (node (ref U5) (pin 16))
      (node (ref J5) (pin 1)))
    (net (code 51) (name /MOSI)
      (node (ref U5) (pin 15))
      (node (ref J5) (pin 4)))
    (net (code 52) (name /Pot_in)
      (node (ref C10) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref U5) (pin 23)))
    (net (code 53) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R8) (pin 2)))
    (net (code 54) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R9) (pin 2)))
    (net (code 55) (name /DAC_out)
      (node (ref U5) (pin 24))
      (node (ref J3) (pin 3))
      (node (ref R13) (pin 1))
      (node (ref C12) (pin 1)))
    (net (code 56) (name /SW_in)
      (node (ref U5) (pin 25))
      (node (ref R10) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref Q1) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 57) (name /#SW_on)
      (node (ref U5) (pin 12))
      (node (ref R12) (pin 1)))
    (net (code 58) (name /SW_out)
      (node (ref Q1) (pin 7))
      (node (ref R5) (pin 1))
      (node (ref Q1) (pin 6))
      (node (ref Q1) (pin 5))
      (node (ref Q1) (pin 8))
      (node (ref J3) (pin 4))
      (node (ref C23) (pin 1))
      (node (ref U5) (pin 26)))
    (net (code 59) (name "Net-(C14-Pad1)")
      (node (ref Y2) (pin 2))
      (node (ref U5) (pin 8))
      (node (ref C14) (pin 1)))
    (net (code 60) (name /MCU_RXD)
      (node (ref U3) (pin 6))
      (node (ref U5) (pin 30)))
    (net (code 61) (name /MCU_TXD)
      (node (ref U3) (pin 7))
      (node (ref U5) (pin 31)))
    (net (code 62) (name /FTDI_TXD)
      (node (ref U3) (pin 3))
      (node (ref U1) (pin 1)))
    (net (code 63) (name /FTDI_RXD)
      (node (ref U1) (pin 5))
      (node (ref U3) (pin 2)))
    (net (code 64) (name "Net-(C13-Pad2)")
      (node (ref C13) (pin 2))
      (node (ref U5) (pin 7))
      (node (ref Y2) (pin 1)))
    (net (code 65) (name /AVCC)
      (node (ref JP3) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref U5) (pin 18)))
    (net (code 66) (name "Net-(U5-Pad19)")
      (node (ref U5) (pin 19)))
    (net (code 67) (name "Net-(U5-Pad22)")
      (node (ref U5) (pin 22)))
    (net (code 68) (name "Net-(Q1-Pad4)")
      (node (ref Q1) (pin 4))
      (node (ref R11) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 69) (name /#PWREN)
      (node (ref U1) (pin 14))
      (node (ref R1) (pin 1)))
    (net (code 70) (name /DAC_VREF)
      (node (ref JP4) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref C18) (pin 2)))
    (net (code 71) (name /AREF)
      (node (ref U5) (pin 20))
      (node (ref JP4) (pin 2))
      (node (ref JP5) (pin 1))
      (node (ref C16) (pin 1)))
    (net (code 72) (name /SDA)
      (node (ref R15) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref U5) (pin 27)))
    (net (code 73) (name /SCL)
      (node (ref U4) (pin 5))
      (node (ref U5) (pin 28))
      (node (ref R14) (pin 2)))))