# FMF Timing for s25fl064p Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 D.Stanojkovic 08 Jan 11 Initial release V1.1 D.Stanojkovic 08 Mar 04 New timmings added and changed timming model labeling V1.2 J.Stoickov 08 Dec 10 Changed timming model labeling V1.3 S.Petrovic 09 May 29 Timing ranges corrected V1.4 V.Mancev 12 Jan 10 Latest datasheet update </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl064p <FMFTIME> S25FL064P0XMFI000_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI001_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI003_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI000_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI001_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI003_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV000_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV001_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV003_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV000_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV001_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV003_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI020_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI023_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI030_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI033_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV020_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV023_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV030_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV033_F_30pF Spansion, S25FL064P_00_05, November 18, 2011 <COMMENT>The values listed are for VCC=2.7V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~dual (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) () (5.4:6.7:8) () (5.4:6.7:8))) (COND dual (IOPATH SCK SO (6.5:8:9.5) (6.5:8:9.5) () (6.5:8:9.5) () (6.5:8:9.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH SCK SI (6.5:8:9.5) (6.5:8:9.5) () (6.5:8:9.5) () (6.5:8:9.5))) (COND dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual && CSNeg (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK HOLDNeg (6.5:8:9.5) (6.5:8:9.5) () (6.5:8:9.5) () (6.5:8:9.5))) (COND dual && CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK WPNeg (6.5:8:9.5) (6.5:8:9.5) () (6.5:8:9.5) () (6.5:8:9.5))) (COND dual && CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) )) (TIMINGCHECK (SETUP CSNeg SCK (3)) (SETUP HOLDNeg SCK (3)) (SETUP SI SCK (3)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (3)) (HOLD HOLDNeg SCK (3)) (HOLD SI SCK (2)) (HOLD WPNeg CSNeg (100)) (WIDTH (COND fast_rd (negedge SCK)) (4.5)) (WIDTH (COND fast_rd (posedge SCK)) (4.5)) (WIDTH (COND dual_rd (negedge SCK)) (4.5)) (WIDTH (COND dual_rd (posedge SCK)) (4.5)) (WIDTH (COND rd (negedge SCK)) (4.5)) (WIDTH (COND rd (posedge SCK)) (4.5)) (WIDTH (COND rd_jid (negedge SCK)) (4.5)) (WIDTH (COND rd_jid (posedge SCK)) (4.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (PERIOD (COND fast_rd SCK) (9.6)) (PERIOD (COND rd SCK) (25.0)) (PERIOD (COND rd_jid SCK) (20.0)) (PERIOD (COND dual_rd SCK) (12.5)) ) </TIMING></FMFTIME> <FMFTIME>
</FTML> <FMFTIME> S25FL064P0XMFI000_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI001_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI003_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI000_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI001_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI003_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV000_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV001_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV003_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV000_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV001_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV003_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI020_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI023_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI030_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI033_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV020_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV023_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV030_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV033_R_30pF Spansion, S25FL064P_00_05, November 18, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~dual (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) () (4.5:5.5:6.5) () (4.5:5.5:6.5))) (COND dual (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) () (5.4:6.7:8) () (5.4:6.7:8))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH SCK SI (5.4:6.7:8) (5.4:6.7:8) () (5.4:6.7:8) () (5.4:6.7:8))) (COND dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual && CSNeg (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK HOLDNeg (5.4:6.7:8) (5.4:6.7:8) () (5.4:6.7:8) () (5.4:6.7:8))) (COND dual && CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK WPNeg (5.4:6.7:8) (5.4:6.7:8) () (5.4:6.7:8) () (5.4:6.7:8))) (COND dual && CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) )) (TIMINGCHECK (SETUP CSNeg SCK (3)) (SETUP HOLDNeg SCK (3)) (SETUP SI SCK (3)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (3)) (HOLD HOLDNeg SCK (3)) (HOLD SI SCK (2)) (HOLD WPNeg CSNeg (100)) (WIDTH (COND fast_rd (negedge SCK)) (4.5)) (WIDTH (COND fast_rd (posedge SCK)) (4.5)) (WIDTH (COND dual_rd (negedge SCK)) (4.5)) (WIDTH (COND dual_rd (posedge SCK)) (4.5)) (WIDTH (COND rd (negedge SCK)) (4.5)) (WIDTH (COND rd (posedge SCK)) (4.5)) (WIDTH (COND rd_jid (negedge SCK)) (4.5)) (WIDTH (COND rd_jid (posedge SCK)) (4.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (PERIOD (COND fast_rd SCK) (9.6)) (PERIOD (COND rd SCK) (25.0)) (PERIOD (COND rd_jid SCK) (20.0)) (PERIOD (COND dual_rd SCK) (12.5)) ) </TIMING></FMFTIME> <FMFTIME> </FTML> <FMFTIME> S25FL064P0XMFI000_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI001_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFI003_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI000_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI001_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFI003_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV000_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV001_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XMFV003_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV000_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV001_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XNFV003_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI020_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI023_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI030_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHI033_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV020_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV023_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV030_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 S25FL064P0XBHV033_R_15pF Spansion, S25FL064P_00_05, November 18, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~dual (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) () (4.5:5.5:6.5) () (4.5:5.5:6.5))) (COND dual (IOPATH SCK SO (4.7:5.8:7) (4.7:5.8:7) () (4.7:5.8:7) () (4.7:5.8:7))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual (IOPATH SCK SI (4.7:5.8:7) (4.7:5.8:7) () (4.7:5.8:7) () (4.7:5.8:7))) (COND dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND dual && CSNeg (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK HOLDNeg (4.7:5.8:7) (4.7:5.8:7) () (4.7:5.8:7) () (4.7:5.8:7))) (COND dual && CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND dual && QUAD (IOPATH SCK WPNeg (4.7:5.8:7) (4.7:5.8:7) () (4.7:5.8:7) () (4.7:5.8:7))) (COND dual && CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) )) (TIMINGCHECK (SETUP CSNeg SCK (3)) (SETUP HOLDNeg SCK (3)) (SETUP SI SCK (3)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (3)) (HOLD HOLDNeg SCK (3)) (HOLD SI SCK (2)) (HOLD WPNeg CSNeg (100)) (WIDTH (COND fast_rd (negedge SCK)) (4.5)) (WIDTH (COND fast_rd (posedge SCK)) (4.5)) (WIDTH (COND dual_rd (negedge SCK)) (4.5)) (WIDTH (COND dual_rd (posedge SCK)) (4.5)) (WIDTH (COND rd (negedge SCK)) (4.5)) (WIDTH (COND rd (posedge SCK)) (4.5)) (WIDTH (COND rd_jid (negedge SCK)) (4.5)) (WIDTH (COND rd_jid (posedge SCK)) (4.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (PERIOD (COND fast_rd SCK) (9.6)) (PERIOD (COND rd SCK) (25.0)) (PERIOD (COND rd_jid SCK) (20.0)) (PERIOD (COND dual_rd SCK) (12.5)) ) </TIMING></FMFTIME> <FMFTIME> </FTML>