# FMF Timing for s25fl128k Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 10 Oct 05 Initial release </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl128k <FMFTIME> S25FL128KOXMFI000 Spansion, S25FL128K, JULY 22,2010 S25FL128KOXMFI001 Spansion, S25FL128K, JULY 22,2010 S25FL128KOXMFI003 Spansion, S25FL128K, JULY 22,2010 <COMMENT>The values listed are for VCC=2.7V to 3.6V, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY(ABSOLUTE (COND RDID == 0 (IOPATH SCK SO (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND RDID == 1 (IOPATH SCK SO (5.5:7:8.5) (5.5:7:8.5) () (5.5:7:8.5) () (5.5:7:8.5))) (IOPATH CSNeg SO () () (5:6:7) () (5:6:7) ()) (IOPATH HOLDNeg SO () () (8:10:12) (5:6:7) (8:10:12) (5:6:7)) )) (TIMINGCHECK (SETUP CSNeg SCK (5)) (SETUP (COND normal SI) (posedge SCK) (2)) (SETUP HOLDNeg SCK (5)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (5)) (HOLD (COND normal SI) (posedge SCK) (5)) (HOLD HOLDNeg SCK (5)) (HOLD WPNeg CSNeg (100)) (WIDTH (COND slow (posedge SCK)) (8)) (WIDTH (COND slow (negedge SCK)) (8)) (WIDTH (COND fast (posedge SCK)) (4)) (WIDTH (COND fast (negedge SCK)) (4)) (WIDTH (COND quad (posedge SCK)) (6)) (WIDTH (COND quad (negedge SCK)) (6)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pger (posedge CSNeg)) (50)) (PERIOD (COND slow SCK) (16)) (PERIOD (COND fast SCK) (8)) (PERIOD (COND quad SCK) (12)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(400000:700000:3000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP1) (DELAY (ABSOLUTE (DEVICE(15000:30000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP2) (DELAY (ABSOLUTE (DEVICE(1000:2500:12000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(10000000:30000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE1) (DELAY (ABSOLUTE (DEVICE(5e7:12e7:8e8) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE2) (DELAY (ABSOLUTE (DEVICE(5e7:15e7:1e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/CE) (DELAY (ABSOLUTE (DEVICE(15e9:25e9:40e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(10000:10000:10000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/DP) (DELAY (ABSOLUTE (DEVICE(3000:3000:3000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/RES1) (DELAY (ABSOLUTE (DEVICE(3000:3000:3000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/RES2) (DELAY (ABSOLUTE (DEVICE(1800:1800:1800) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGRES) (DELAY (ABSOLUTE (DEVICE(200:200:200) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSRES) (DELAY (ABSOLUTE (DEVICE(200:200:200) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(15000000:15000000:15000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SUSP_DLY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME>
</FTML>