# FMF Timing for s25fl256s Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 09 Nov 27 Initial release V1.1 V.Mancev 10 Oct 20 Latest datasheet aligned V1.2 B.Colakovic 11 June 29 Latest datasheet aligned V1.3 V.Mancev 11 Nov 17 Time tHO is changed to 1 ns </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl256s <FMFTIME> S25FL256SAGMFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for VIO=VCC=2.7V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME>
</FTML> <FMFTIME> S25FL256SAGMFI000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR01_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR01_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI200_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI203_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI300_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI303_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV200_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV203_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV300_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV303_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL256SAGMFI000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR01_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFIR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR01_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGMFVR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGNFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI200_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI203_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI300_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI303_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHI313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHID13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV200_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV203_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV300_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV303_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHV313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHVD13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIY13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIZ13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIS13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIT13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIK13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SAGBHIL13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL256SDPMFIR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL256SDPMFIR00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR01_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR11_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPMFIR13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI000_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI001_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI003_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI010_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI011_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPNFI013_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI200_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI203_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI210_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI213_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI300_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI303_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI310_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHI313_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHIC13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL256SDPBHID13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML>