# FMF Timing for s25fl128s Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 09 Nov 19 Initial release V1.1 V.Mancev 10 Oct 07 Latest datasheet aligned V1.2 V.Mancev 11 May 11 CS# High Time modifications V1.3 V.Mancev 11 June 27 Latest datasheet aligned V1.4 V.Mancev 11 Nov 16 Time tHO is changed to 1 ns </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl128s <FMFTIME> S25FL128SAGMFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for VIO=VCC=2.7V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME>
</FTML> <FMFTIME> S25FL128SAGMFI000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR01_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR01_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV000_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV001_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV003_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI200_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI203_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI300_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI303_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV200_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV203_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV300_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV303_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL00_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL03_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL128SAGMFI000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR01_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFIR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR01_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGMFVR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV000_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV001_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV003_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGNFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI200_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI203_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI300_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI303_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHI313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHID13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV200_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV203_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV300_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV303_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHV313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHVD13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIY13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIZ13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIS13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIT13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIK13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL00_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL03_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SAGBHIL13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL128SDPMFIR00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR01_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI000_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI001_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI003_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI200_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI203_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI300_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI303_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID00_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID03_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL128SDPMFIR00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR01_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR11_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPMFIR13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI000_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI001_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI003_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI010_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI011_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPNFI013_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI200_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI203_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI210_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI213_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI300_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI303_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI310_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHI313_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHIC13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID00_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID03_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL128SDPBHID13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML>