# FMF Timing for s25fl064k Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 10 Sep 11 Initial release </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl064k <FMFTIME> S25FL064KOSMFI000 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI001 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI003 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI010 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI011 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI013 Spansion, S25FL064K, Rev. 01,JUN.29,2010 <COMMENT>The values listed are for VCC=2.7V to 3.6V, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY(ABSOLUTE (COND RDID == 0 (IOPATH SCK SO (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND RDID == 1 (IOPATH SCK SO (5.5:7:8.5) (5.5:7:8.5) () (5.5:7:8.5) () (5.5:7:8.5))) (IOPATH CSNeg SO () () (5:6:7) () (5:6:7) ()) (IOPATH HOLDNeg SO () () (8:10:12) (5:6:7) (8:10:12) (5:6:7)) )) (TIMINGCHECK (SETUP CSNeg SCK (5)) (SETUP (COND normal SI) (posedge SCK) (2)) (SETUP HOLDNeg SCK (5)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (5)) (HOLD (COND normal SI) (posedge SCK) (5)) (HOLD HOLDNeg SCK (5)) (HOLD WPNeg CSNeg (100)) (WIDTH (COND slow (posedge SCK)) (15.2)) (WIDTH (COND slow (negedge SCK)) (15.2)) (WIDTH (COND fast (posedge SCK)) (6.25)) (WIDTH (COND fast (negedge SCK)) (6.25)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pger (posedge CSNeg)) (50)) (PERIOD (COND slow SCK) (30.4)) (PERIOD (COND fast SCK) (12.5)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(400000:700000:3000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP1) (DELAY (ABSOLUTE (DEVICE(15000:30000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP2) (DELAY (ABSOLUTE (DEVICE(1000:2500:12000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(10000000:30000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE1) (DELAY (ABSOLUTE (DEVICE(5e7:12e7:8e8) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE2) (DELAY (ABSOLUTE (DEVICE(5e7:15e7:1e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/CE) (DELAY (ABSOLUTE (DEVICE(5e9:15e9:30e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(10000:10000:10000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/DP) (DELAY (ABSOLUTE (DEVICE(3000:3000:3000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/RES1) (DELAY (ABSOLUTE (DEVICE(3000:3000:3000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/RES2) (DELAY (ABSOLUTE (DEVICE(1800:1800:1800) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGRES) (DELAY (ABSOLUTE (DEVICE(200:200:200) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSRES) (DELAY (ABSOLUTE (DEVICE(200:200:200) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(15000000:15000000:15000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SUSP_DLY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME>
</FTML>