# FMF Timing for s25fl512s Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 V.Mancev 09 Nov 26 Initial release V1.1 V.Mancev 11 July 11 Latest datasheet aligned V1.2 V.Mancev 11 Nov 17 Time tHO is changed to 1 ns </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl512s <FMFTIME> S25FL512SAGMFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for VCC=2.7V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND normal (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND DDR (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ()) (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP (COND normal CSNeg) (posedge SCK) (3)) (SETUP (COND DDR CSNeg) (posedge SCK) (3)) (SETUP (COND normal SI) (posedge SCK) (3)) (SETUP WPNeg CSNeg (20)) (SETUP HOLDNeg SCK (3)) (SETUP RSTNeg CSNeg (50)) (SETUP (COND DDR SI) (posedge SCK) (2)) (SETUP (COND DDR SI) (negedge SCK) (2)) (HOLD (COND normal CSNeg) (posedge SCK) (3)) (HOLD (COND DDR CSNeg) (posedge SCK) (3)) (HOLD (COND normal SI) (posedge SCK) (2)) (HOLD WPNeg CSNeg (100)) (HOLD HOLDNeg SCK (3)) (HOLD CSNeg RSTNeg (35000)) (HOLD (COND DDR SI) (posedge SCK) (2)) (HOLD (COND DDR SI) (negedge SCK) (2)) (WIDTH (COND serial (posedge SCK)) (10)) (WIDTH (COND serial (negedge SCK)) (10)) (WIDTH (COND dual (posedge SCK)) (4.8)) (WIDTH (COND dual (negedge SCK)) (4.8)) (WIDTH (COND fast (negedge SCK)) (3.75)) (WIDTH (COND fast (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND DDR (posedge SCK)) (7.5)) (WIDTH (COND DDR (negedge SCK)) (7.5)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pgers (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND serial_rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND DDR_rd SCK) (15)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(200e3:340e3:750e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP) (DELAY (ABSOLUTE (DEVICE(100e3:150e3:400e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(200e6:400e6:1875e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE) (DELAY (ABSOLUTE (DEVICE(55e9:103e9:460e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(200e6:200e6:200e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(300e3:300e3:300e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PPBERASE) (DELAY (ABSOLUTE (DEVICE(15e6:15e6:15e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSULCK) (DELAY (ABSOLUTE (DEVICE(1000:1000:1000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSACC) (DELAY (ABSOLUTE (DEVICE(100e3:100e3:100e3) ) ) ) </TIMING></FMFTIME>
</FTML> <FMFTIME> S25FL512SAGMFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND normal (IOPATH SCK SO (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND DDR (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ()) (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP (COND normal CSNeg) (posedge SCK) (3)) (SETUP (COND DDR CSNeg) (posedge SCK) (3)) (SETUP (COND normal SI) (posedge SCK) (3)) (SETUP WPNeg CSNeg (20)) (SETUP HOLDNeg SCK (3)) (SETUP RSTNeg CSNeg (50)) (SETUP (COND DDR SI) (posedge SCK) (2)) (SETUP (COND DDR SI) (negedge SCK) (2)) (HOLD (COND normal CSNeg) (posedge SCK) (3)) (HOLD (COND DDR CSNeg) (posedge SCK) (3)) (HOLD (COND normal SI) (posedge SCK) (2)) (HOLD WPNeg CSNeg (100)) (HOLD HOLDNeg SCK (3)) (HOLD CSNeg RSTNeg (35000)) (HOLD (COND DDR SI) (posedge SCK) (2)) (HOLD (COND DDR SI) (negedge SCK) (2)) (WIDTH (COND serial (posedge SCK)) (10)) (WIDTH (COND serial (negedge SCK)) (10)) (WIDTH (COND dual (posedge SCK)) (4.8)) (WIDTH (COND dual (negedge SCK)) (4.8)) (WIDTH (COND fast (negedge SCK)) (3.75)) (WIDTH (COND fast (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND DDR (posedge SCK)) (7.5)) (WIDTH (COND DDR (negedge SCK)) (7.5)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pgers (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND serial_rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND DDR_rd SCK) (15)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(200e3:340e3:750e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP) (DELAY (ABSOLUTE (DEVICE(100e3:150e3:400e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(200e6:400e6:1875e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE) (DELAY (ABSOLUTE (DEVICE(55e9:103e9:460e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(200e6:200e6:200e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(300e3:300e3:300e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PPBERASE) (DELAY (ABSOLUTE (DEVICE(15e6:15e6:15e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSULCK) (DELAY (ABSOLUTE (DEVICE(1000:1000:1000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSACC) (DELAY (ABSOLUTE (DEVICE(100e3:100e3:100e3) ) ) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SAGMFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND normal (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND DDR (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ()) (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP (COND normal CSNeg) (posedge SCK) (3)) (SETUP (COND DDR CSNeg) (posedge SCK) (3)) (SETUP (COND normal SI) (posedge SCK) (3)) (SETUP WPNeg CSNeg (20)) (SETUP HOLDNeg SCK (3)) (SETUP RSTNeg CSNeg (50)) (SETUP (COND DDR SI) (posedge SCK) (2)) (SETUP (COND DDR SI) (negedge SCK) (2)) (HOLD (COND normal CSNeg) (posedge SCK) (3)) (HOLD (COND DDR CSNeg) (posedge SCK) (3)) (HOLD (COND normal SI) (posedge SCK) (2)) (HOLD WPNeg CSNeg (100)) (HOLD HOLDNeg SCK (3)) (HOLD CSNeg RSTNeg (35000)) (HOLD (COND DDR SI) (posedge SCK) (2)) (HOLD (COND DDR SI) (negedge SCK) (2)) (WIDTH (COND serial (posedge SCK)) (10)) (WIDTH (COND serial (negedge SCK)) (10)) (WIDTH (COND dual (posedge SCK)) (4.8)) (WIDTH (COND dual (negedge SCK)) (4.8)) (WIDTH (COND fast (negedge SCK)) (3.75)) (WIDTH (COND fast (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND DDR (posedge SCK)) (7.5)) (WIDTH (COND DDR (negedge SCK)) (7.5)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pgers (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND serial_rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND DDR_rd SCK) (15)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(200e3:340e3:750e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP) (DELAY (ABSOLUTE (DEVICE(100e3:150e3:400e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(200e6:400e6:1875e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE) (DELAY (ABSOLUTE (DEVICE(55e9:103e9:460e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(200e6:200e6:200e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(300e3:300e3:300e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PPBERASE) (DELAY (ABSOLUTE (DEVICE(15e6:15e6:15e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSULCK) (DELAY (ABSOLUTE (DEVICE(1000:1000:1000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSACC) (DELAY (ABSOLUTE (DEVICE(100e3:100e3:100e3) ) ) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SDPMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND normal (IOPATH SCK SO (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND DDR (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ()) (IOPATH HOLDNeg SO () () (10:12:14) (10:12:14) (10:12:14) (10:12:14)) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP (COND normal CSNeg) (posedge SCK) (3)) (SETUP (COND DDR CSNeg) (posedge SCK) (3)) (SETUP (COND normal SI) (posedge SCK) (5)) (SETUP WPNeg CSNeg (20)) (SETUP HOLDNeg SCK (5)) (SETUP RSTNeg CSNeg (50)) (SETUP (COND DDR SI) (posedge SCK) (2)) (SETUP (COND DDR SI) (negedge SCK) (2)) (HOLD (COND normal CSNeg) (posedge SCK) (3)) (HOLD (COND DDR CSNeg) (posedge SCK) (3)) (HOLD (COND normal SI) (posedge SCK) (4)) (HOLD WPNeg CSNeg (100)) (HOLD HOLDNeg SCK (5)) (HOLD CSNeg RSTNeg (35000)) (HOLD (COND DDR SI) (posedge SCK) (2)) (HOLD (COND DDR SI) (negedge SCK) (2)) (WIDTH (COND serial (posedge SCK)) (10)) (WIDTH (COND serial (negedge SCK)) (10)) (WIDTH (COND dual (posedge SCK)) (7.5)) (WIDTH (COND dual (negedge SCK)) (7.5)) (WIDTH (COND fast (negedge SCK)) (7.5)) (WIDTH (COND fast (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND DDR (posedge SCK)) (7.5)) (WIDTH (COND DDR (negedge SCK)) (7.5)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pgers (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND serial_rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND DDR_rd SCK) (15)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(200e3:340e3:750e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP) (DELAY (ABSOLUTE (DEVICE(100e3:150e3:400e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(200e6:400e6:1875e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE) (DELAY (ABSOLUTE (DEVICE(55e9:103e9:460e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(200e6:200e6:200e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(300e3:300e3:300e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PPBERASE) (DELAY (ABSOLUTE (DEVICE(15e6:15e6:15e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSULCK) (DELAY (ABSOLUTE (DEVICE(1000:1000:1000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSACC) (DELAY (ABSOLUTE (DEVICE(100e3:100e3:100e3) ) ) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SDPMFIR10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR11_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI210_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI213_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI310_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI313_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND normal (IOPATH SCK SO (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND DDR (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ()) (IOPATH HOLDNeg SO () () (10:12:14) (10:12:14) (10:12:14) (10:12:14)) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP (COND normal CSNeg) (posedge SCK) (3)) (SETUP (COND DDR CSNeg) (posedge SCK) (3)) (SETUP (COND normal SI) (posedge SCK) (5)) (SETUP WPNeg CSNeg (20)) (SETUP HOLDNeg SCK (5)) (SETUP RSTNeg CSNeg (50)) (SETUP (COND DDR SI) (posedge SCK) (2)) (SETUP (COND DDR SI) (negedge SCK) (2)) (HOLD (COND normal CSNeg) (posedge SCK) (3)) (HOLD (COND DDR CSNeg) (posedge SCK) (3)) (HOLD (COND normal SI) (posedge SCK) (4)) (HOLD WPNeg CSNeg (100)) (HOLD HOLDNeg SCK (5)) (HOLD CSNeg RSTNeg (35000)) (HOLD (COND DDR SI) (posedge SCK) (2)) (HOLD (COND DDR SI) (negedge SCK) (2)) (WIDTH (COND serial (posedge SCK)) (10)) (WIDTH (COND serial (negedge SCK)) (10)) (WIDTH (COND dual (posedge SCK)) (7.5)) (WIDTH (COND dual (negedge SCK)) (7.5)) (WIDTH (COND fast (negedge SCK)) (7.5)) (WIDTH (COND fast (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND DDR (posedge SCK)) (7.5)) (WIDTH (COND DDR (negedge SCK)) (7.5)) (WIDTH (COND read (posedge CSNeg)) (10)) (WIDTH (COND pgers (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND serial_rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND DDR_rd SCK) (15)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PP) (DELAY (ABSOLUTE (DEVICE(200e3:340e3:750e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BP) (DELAY (ABSOLUTE (DEVICE(100e3:150e3:400e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/SE) (DELAY (ABSOLUTE (DEVICE(200e6:400e6:1875e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/BE) (DELAY (ABSOLUTE (DEVICE(55e9:103e9:460e9) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/WRR) (DELAY (ABSOLUTE(DEVICE(200e6:200e6:200e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PU) (DELAY (ABSOLUTE (DEVICE(300e3:300e3:300e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PRGSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/ERSSUSP) (DELAY (ABSOLUTE (DEVICE(40e3:40e3:40e3) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PPBERASE) (DELAY (ABSOLUTE (DEVICE(15e6:15e6:15e6) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSULCK) (DELAY (ABSOLUTE (DEVICE(1000:1000:1000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE %LABEL%/PASSACC) (DELAY (ABSOLUTE (DEVICE(100e3:100e3:100e3) ) ) ) </TIMING></FMFTIME> </FTML>