# FMF Timing for s25fl512s Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 09 Nov 27 Initial release V1.1 V.Mancev 10 Oct 20 Latest datasheet aligned V1.2 B.Colakovic 11 July 11 Latest datasheet aligned V1.3 V.Mancev 11 Nov 17 Time tHO is changed to 1 ns </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl512s <FMFTIME> S25FL512SAGMFI010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for VIO=VCC=2.7V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (5.4:6.7:8) (5.4:6.7:8) (1) (5.4:6.7:8) (1) (5.4:6.7:8))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME>
</FTML> <FMFTIME> S25FL512SAGMFI010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_R_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=30pF </COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.3:6.0:7.65) (4.3:6.0:7.65) (1) (4.3:6.0:7.65) (1) (4.3:6.0:7.65))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SAGMFI010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFI013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFIR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV010_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV011_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFV013_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR11_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGMFVR13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHI313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHID13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV210_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV213_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV310_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHV313_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVA13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVB13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVC13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHVD13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIY13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIZ13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIS13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIT13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIK13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL10_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SAGBHIL13_R_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for regulated Vcc range VCC=3.0V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (4.5:5.5:6.5) (4.5:5.5:6.5) (1) (4.5:5.5:6.5) (1) (4.5:5.5:6.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (3)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (3)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (2)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (3)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (4.8)) (WIDTH (COND dual_rd (negedge SCK)) (4.8)) (WIDTH (COND fast_rd (negedge SCK)) (3.75)) (WIDTH (COND fast_rd (posedge SCK)) (3.75)) (WIDTH (COND quadpg (posedge SCK)) (6.25)) (WIDTH (COND quadpg (negedge SCK)) (6.25)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (7.52)) (PERIOD (COND dual_rd SCK) (9.6)) (PERIOD (COND quadpg SCK) (12.5)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SDPMFIR10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR11_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI210_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI213_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI310_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI313_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID10_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID13_F_30pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=30pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (1.5:8:14.5) (1.5:8:14.5) (1) (1.5:8:14.5) (1) (1.5:8:14.5))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML> <FMFTIME> S25FL512SDPMFIR10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR11_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPMFIR13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI210_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI213_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI310_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHI313_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHIC13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID10_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 S25FL512SDPBHID13_F_15pF Spansion, FL-S_PPD_2.0 April 1, 2011 <COMMENT>The values listed are for Vcc range VCC=2.7V to 3.6V, CL=15pF, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY (ABSOLUTE (COND ~ddr (IOPATH SCK SO (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND (ddr || rd_fast) (IOPATH SCK SO (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && dual (IOPATH SCK SI (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && dual (IOPATH SCK SI (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK HOLDNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK HOLDNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND ~ddr && QUAD (IOPATH SCK WPNeg (2:7:12) (2:7:12) (1) (2:7:12) (1) (2:7:12))) (COND ddr && QUAD (IOPATH SCK WPNeg (1.5:4:6.5) (1.5:4:6.5) (1) (1.5:4:6.5) (1) (1.5:4:6.5))) (COND CSNeg (IOPATH CSNeg SO () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && dual (IOPATH CSNeg SI () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg HOLDNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND CSNeg && QUAD (IOPATH CSNeg WPNeg () () (5.4:6.7:8) () (5.4:6.7:8) ())) (COND ~QUAD (IOPATH HOLDNeg SO () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (COND ~QUAD && dual (IOPATH HOLDNeg SI () () (7:10.5:14) (7:10.5:14) (7:10.5:14) (7:10.5:14))) (IOPATH RSTNeg SO () () (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8) (5.4:6.7:8)) )) (TIMINGCHECK (SETUP CSNeg (COND sdr_rd SCK) (3)) (SETUP CSNeg (COND ddr_rd SCK) (3)) (SETUP SI (COND deg_sin(posedge SCK)) (5)) (SETUP SI (COND ddro(posedge SCK)) (2)) (SETUP SI (COND ddro(negedge SCK)) (2)) (SETUP WPNeg (COND wr_prot(negedge CSNeg)) (20)) (SETUP HOLDNeg (COND quad_rd (posedge SCK)) (5)) (SETUP RSTNeg CSNeg (50)) (HOLD CSNeg (COND sdr_rd SCK) (3)) (HOLD CSNeg (COND ddr_rd SCK) (3)) (HOLD SI (COND deg_sin (posedge SCK)) (4)) (HOLD SI (COND ddro (posedge SCK)) (2)) (HOLD SI (COND ddro (negedge SCK)) (2)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (HOLD HOLDNeg (COND quad_rd (posedge SCK)) (5)) (HOLD CSNeg RSTNeg (35000)) (WIDTH (COND rd (posedge SCK)) (10)) (WIDTH (COND rd (negedge SCK)) (10)) (WIDTH (COND dual_rd (posedge SCK)) (7.5)) (WIDTH (COND dual_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (negedge SCK)) (7.5)) (WIDTH (COND fast_rd (posedge SCK)) (7.5)) (WIDTH (COND quadpg (posedge SCK)) (7.5)) (WIDTH (COND quadpg (negedge SCK)) (7.5)) (WIDTH (COND ddrd (posedge SCK)) (7.5)) (WIDTH (COND ddrd (negedge SCK)) (7.5)) (WIDTH (COND RD_EQU_1 (posedge CSNeg)) (10)) (WIDTH (COND RD_EQU_0 (posedge CSNeg)) (50)) (WIDTH (negedge RSTNeg) (200)) (WIDTH (posedge RSTNeg) (50)) (PERIOD (COND rd SCK) (20)) (PERIOD (COND fast_rd SCK) (15)) (PERIOD (COND dual_rd SCK) (15)) (PERIOD (COND quadpg SCK) (15)) (PERIOD (COND ddrd SCK) (15)) ) </TIMING></FMFTIME> </FTML>