# FMF Timing for s25fl064k Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 R. Prokopovic 10 Aug 25 Initial release </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>s25fl064k <FMFTIME> S25FL064KOSMFI000 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI001 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI003 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI010 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI011 Spansion, S25FL064K, Rev. 01,JUN.29,2010 S25FL064KOSMFI013 Spansion, S25FL064K, Rev. 01,JUN.29,2010 <COMMENT>The values listed are for VCC=2.7V to 3.6V, Industrial Ta=-40 to +85 Celsius</COMMENT> <TIMING> (DELAY(ABSOLUTE (COND ~read_id (IOPATH SCK SO (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND read_id (IOPATH SCK SO (5.5:7:8.5) (5.5:7:8.5) () (5.5:7:8.5) () (5.5:7:8.5))) (COND CSNeg (IOPATH CSNeg SO () () (5:6:7) () (5:6:7) ())) (COND ~quad_read (IOPATH HOLDNeg SO () () (8:10:12) (5:6:7) (8:10:12) (5:6:7))) (COND dual_read || quad_read (IOPATH SCK SI (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND CSNeg && ~deg_sin (IOPATH CSNeg SI () () (5:6:7) () (5:6:7) ())) (COND ~quad_read && dual_read (IOPATH HOLDNeg SI () () (8:10:12) (5:6:7) (8:10:12) (5:6:7))) (COND quad_read (IOPATH SCK WPNeg (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND quad_read (IOPATH SCK HOLDNeg (5:6:7) (5:6:7) () (5:6:7) () (5:6:7))) (COND CSNeg && QE (IOPATH CSNeg SI () () (5:6:7) () (5:6:7) ())) (COND CSNeg && QE (IOPATH CSNeg WPNeg () () (5:6:7) () (5:6:7) ())) (COND CSNeg && QE (IOPATH CSNeg HOLDNeg () () (5:6:7) () (5:6:7) ())) )) (TIMINGCHECK (SETUP CSNeg (posedge SCK) (5)) (SETUP SI (COND deg_sin(posedge SCK)) (2)) (SETUP SO (COND quad_pg(posedge SCK)) (2)) (SETUP WPNeg (COND quad_pg(posedge SCK)) (2)) (SETUP HOLDNeg (COND quad_pg(posedge SCK)) (2)) (SETUP HOLDNeg (COND hold_cond(posedge SCK)) (5)) (SETUP WPNeg CSNeg (20)) (HOLD CSNeg SCK (5)) (HOLD SI (COND deg_sin (posedge SCK)) (5)) (HOLD SO (COND quad_pg (posedge SCK)) (5)) (HOLD WPNeg (COND quad_pg (posedge SCK)) (5)) (HOLD HOLDNeg (COND quad_pg (posedge SCK)) (5)) (HOLD HOLDNeg (COND hold_cond(posedge SCK)) (5)) (HOLD WPNeg (COND wr_prot (posedge CSNeg)) (100)) (WIDTH (COND rd_slow (posedge SCK)) (15.2)) (WIDTH (COND rd_slow (negedge SCK)) (15.2)) (WIDTH (COND rd_fast (posedge SCK)) (6.25)) (WIDTH (COND rd_fast (negedge SCK)) (6.25)) (WIDTH (COND any_read (posedge CSNeg)) (10)) (WIDTH (COND pg_ers (posedge CSNeg)) (50)) (PERIOD (COND rd_slow SCK) (30.4)) (PERIOD (COND rd_fast SCK) (12.5)) ) </TIMING></FMFTIME>
</FTML>