# FMF Timing for testbench Parts

<FTML>
<REVISION.HISTORY> version: | author: | mod date: | changes made: V1.0 VHD2FTM 03 July 11 Initial release </REVISION.HISTORY> <TIMESCALE>1ns</TIMESCALE> <MODEL>am29lv640m <FMFTIME> MY_MEM AM29LV640MH90R AM29LV640ML90R <COMMENT></COMMENT> <TIMING> (DELAY (ABSOLUTE (IOPATH A0 DQ0 (90:90:90) (90:90:90)) (IOPATH A0 DQ1 (25:25:25) (25:25:25)) (IOPATH CENeg DQ0 (85:85:85) (85:85:85) (11:11:11) (85:85:85) (11:11:11) (85:85:85)) (IOPATH OENeg DQ0 (20:20:20) (20:20:20) (11:11:11) (20:20:20) (11:11:11) (20:20:20)) (IOPATH RESETNeg DQ0 () () (0:0:0) () (0:0:0) ()) (IOPATH CENeg RY (0) (90)) (IOPATH WENeg RY (0) (90)) )) (TIMINGCHECK (SETUP A0 CENeg (0:0:0)) (SETUP A0 OENeg (15:15:15)) (SETUP DQ0 CENeg (45:45:45)) (HOLD CENeg RESETNeg (50:50:50)) (HOLD OENeg WENeg (0:0:0)) (HOLD A0 CENeg (45:45:45)) (HOLD A0 OENeg (0:0:0)) (HOLD DQ0 CENeg (0:0:0)) (HOLD WENeg OENeg (0:0:0)) (WIDTH (negedge RESETNeg) (500:500:500)) (WIDTH (posedge OENeg) (20:20:20)) (WIDTH (negedge WENeg) (35:35:35)) (WIDTH (posedge WENeg) (30:30:30)) (WIDTH (negedge CENeg) (45:45:45)) (WIDTH (posedge CENeg) (30:30:30)) (WIDTH (negedge A0) (90:90:90)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/WBPB) (DELAY (ABSOLUTE (DEVICE(11000:11000:11000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/POB) (DELAY (ABSOLUTE (DEVICE(100000:100000:100000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/SEO) (DELAY (ABSOLUTE (DEVICE(500000000:500000000:500000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/HANG) (DELAY (ABSOLUTE (DEVICE(400000000:400000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/START_T1) (DELAY (ABSOLUTE (DEVICE(5000:5000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/CTMOUT) (DELAY (ABSOLUTE (DEVICE(50000:50000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/READY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME> <FMFTIME> AM29LV640MH101 AM29LV640ML101 AM29LV640MH101R AM29LV640ML101R <COMMENT></COMMENT> <TIMING> (DELAY (ABSOLUTE (IOPATH A0 DQ0 (100:100:100) (100:100:100)) (IOPATH A0 DQ1 (30:30:30) (30:30:30)) (IOPATH CENeg DQ0 (95:95:95) (95:95:95) (11:11:11) (95:95:95) (11:11:11) (95:95:95)) (IOPATH OENeg DQ0 (25:25:25) (25:25:25) (11:11:11) (25:25:25) (11:11:11) (25:25:25)) (IOPATH RESETNeg DQ0 () () (0:0:0) () (0:0:0) ()) (IOPATH CENeg RY (0) (100)) (IOPATH WENeg RY (0) (100)) )) (TIMINGCHECK (SETUP A0 CENeg (0:0:0)) (SETUP A0 OENeg (15:15:15)) (SETUP DQ0 CENeg (45:45:45)) (HOLD CENeg RESETNeg (50:50:50)) (HOLD OENeg WENeg (0:0:0)) (HOLD A0 CENeg (45:45:45)) (HOLD A0 OENeg (0:0:0)) (HOLD DQ0 CENeg (0:0:0)) (HOLD WENeg OENeg (0:0:0)) (WIDTH (negedge RESETNeg) (500:500:500)) (WIDTH (posedge OENeg) (20:20:20)) (WIDTH (negedge WENeg) (35:35:35)) (WIDTH (posedge WENeg) (30:30:30)) (WIDTH (negedge CENeg) (45:45:45)) (WIDTH (posedge CENeg) (30:30:30)) (WIDTH (negedge A0) (100:100:100)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/WBPB) (DELAY (ABSOLUTE (DEVICE(11000:11000:11000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/POB) (DELAY (ABSOLUTE (DEVICE(100000:100000:100000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/SEO) (DELAY (ABSOLUTE (DEVICE(500000000:500000000:500000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/HANG) (DELAY (ABSOLUTE (DEVICE(400000000:400000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/START_T1) (DELAY (ABSOLUTE (DEVICE(5000:5000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/CTMOUT) (DELAY (ABSOLUTE (DEVICE(50000:50000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/READY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME> <FMFTIME> AM29LV640MH112 AM29LV640ML112 AM29LV640MH112R AM29LV640ML112R <COMMENT></COMMENT> <TIMING> (DELAY (ABSOLUTE (IOPATH A0 DQ0 (110:110:110) (110:110:110)) (IOPATH A0 DQ1 (40:40:40) (40:40:40)) (IOPATH CENeg DQ0 (105:105:105) (105:105:105) (11:11:11) (105:105:105) (11:11:11) (105:105:105)) (IOPATH OENeg DQ0 (35:35:35) (35:35:35) (11:11:11) (35:35:35) (11:11:11) (35:35:35)) (IOPATH RESETNeg DQ0 () () (0:0:0) () (0:0:0) ()) (IOPATH CENeg RY (0) (110)) (IOPATH WENeg RY (0) (110)) )) (TIMINGCHECK (SETUP A0 CENeg (0:0:0)) (SETUP A0 OENeg (15:15:15)) (SETUP DQ0 CENeg (45:45:45)) (HOLD CENeg RESETNeg (50:50:50)) (HOLD OENeg WENeg (0:0:0)) (HOLD A0 CENeg (45:45:45)) (HOLD A0 OENeg (0:0:0)) (HOLD DQ0 CENeg (0:0:0)) (HOLD WENeg OENeg (0:0:0)) (WIDTH (negedge RESETNeg) (500:500:500)) (WIDTH (posedge OENeg) (20:20:20)) (WIDTH (negedge WENeg) (35:35:35)) (WIDTH (posedge WENeg) (30:30:30)) (WIDTH (negedge CENeg) (45:45:45)) (WIDTH (posedge CENeg) (30:30:30)) (WIDTH (negedge A0) (110:110:110)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/WBPB) (DELAY (ABSOLUTE (DEVICE(11000:11000:11000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/POB) (DELAY (ABSOLUTE (DEVICE(100000:100000:100000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/SEO) (DELAY (ABSOLUTE (DEVICE(500000000:500000000:500000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/HANG) (DELAY (ABSOLUTE (DEVICE(400000000:400000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/START_T1) (DELAY (ABSOLUTE (DEVICE(5000:5000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/CTMOUT) (DELAY (ABSOLUTE (DEVICE(50000:50000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/READY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME> <FMFTIME> AM29LV640MH120 AM29LV640ML120 AM29LV640MH120R AM29LV640ML120R <COMMENT></COMMENT> <TIMING> (DELAY (ABSOLUTE (IOPATH A0 DQ0 (120:120:120) (120:120:120)) (IOPATH A0 DQ1 (40:40:40) (40:40:40)) (IOPATH CENeg DQ0 (115:115:115) (115:115:115) (11:11:11) (115:115:115) (11:11:11) (115:115:115)) (IOPATH OENeg DQ0 (35:35:35) (35:35:35) (11:11:11) (35:35:35) (11:11:11) (35:35:35)) (IOPATH RESETNeg DQ0 () () (0:0:0) () (0:0:0) ()) (IOPATH CENeg RY (0) (120)) (IOPATH WENeg RY (0) (120)) )) (TIMINGCHECK (SETUP A0 CENeg (0:0:0)) (SETUP A0 OENeg (15:15:15)) (SETUP DQ0 CENeg (45:45:45)) (HOLD CENeg RESETNeg (50:50:50)) (HOLD OENeg WENeg (0:0:0)) (HOLD A0 CENeg (45:45:45)) (HOLD A0 OENeg (0:0:0)) (HOLD DQ0 CENeg (0:0:0)) (HOLD WENeg OENeg (0:0:0)) (WIDTH (negedge RESETNeg) (500:500:500)) (WIDTH (posedge OENeg) (20:20:20)) (WIDTH (negedge WENeg) (35:35:35)) (WIDTH (posedge WENeg) (30:30:30)) (WIDTH (negedge CENeg) (45:45:45)) (WIDTH (posedge CENeg) (30:30:30)) (WIDTH (negedge A0) (120:120:120)) )) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/WBPB) (DELAY (ABSOLUTE (DEVICE(11000:11000:11000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/POB) (DELAY (ABSOLUTE (DEVICE(100000:100000:100000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/SEO) (DELAY (ABSOLUTE (DEVICE(500000000:500000000:500000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/HANG) (DELAY (ABSOLUTE (DEVICE(400000000:400000000:400000000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/START_T1) (DELAY (ABSOLUTE (DEVICE(5000:5000:20000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/CTMOUT) (DELAY (ABSOLUTE (DEVICE(50000:50000:50000) ) ) ) ) (CELL (CELLTYPE "VITALbuf") (INSTANCE dut/READY) (DELAY (ABSOLUTE (DEVICE(20000:20000:20000) ) ) ) </TIMING></FMFTIME>
</FTML>